|  |
| --- |
| Queensland Recreational Boating Facilities Demand Forecasting Study 2022  Western Downs Region Assessment |
|  |
|  |

|  |  |  |
| --- | --- | --- |
| Customer |  | Maritime Safety Queensland |
| Project |  | A12068 |
| Deliverable |  | 038 |
| Version |  | 01 |
|  |  | 21 April 2023 |

Document Control

Document Identification

|  |  |
| --- | --- |
| Title | Queensland Recreational Boating Facilities Demand Forecasting Study 2022 |
| Project No | A12068 |
| Deliverable No | 038 |
| Version No | 01 |
| Version Date | 21 April 2023 |
| Customer | Maritime Safety Queensland, a branch of the Department of Transport and Main Roads |
| Customer Contact | boatinginfrastructure@msq.qld.gov.au |
| Classification | {None} |

|  |  |
| --- | --- |
| Author | Daniel Wishaw, Nicholas Heiner, Geoff Long, Sophie Barrett, Mackenzie Stacey |
| Reviewed By | Katrina O’Malley-Jones, Jeremy Visser, Matthew Barnes |
| Project Manager | Daniel Wishaw |

Amendment Record

The Amendment Record below records the history and issue status of this document.

| Version | Version Date | Distribution | Record |
| --- | --- | --- | --- |
| 00 | 06 December 2022 | Maritime Safety Queensland Western Downs Region Council | Draft |
| 01 | 21 April 2023 | Maritime Safety Queensland | Final |

Executive Summary

This report, part of the Queensland Recreational Boating Facilities Demand Forecasting Study 2022 (‘the Study’), provides a summary of current and forecast demand on recreational boating facilities in the Western Downs LGA and the capacity of existing facilities to meet this demand. Where capacity is insufficient to meet current or forecast demand, recommendations have been made to improve existing facilities or for the construction of new facilities. This report is intended to support facility deliverers, owners, and managers over the next 20 years in their decision-making on development priorities for recreational boating facilities within the Western Downs LGA.

Key issues and attributes of recreational boating

The key attributes of recreational boating facilities identified in this Study for the Western Downs LGA are summarised in Table 1, while consultation with stakeholders undertaken as part of the Study identified the following key issues:

* Water level fluctuations impacts the ability to access most water bodies across the LGA
* The number of boats permitted on the water bodies effectively constrains the capacity, rather than the facilities that access them.

1. Key recreational boating attributes for the Western Downs LGA

| Key attribute | Value |
| --- | --- |
| Boat launching facilities |  |
| Number of existing facilities | 3 |
| Current demand for boat launching lanes (effective lanes) | 1.1 |
| Number of existing ‘effective’ boat launching lanes | 2.8 |
| Shortfall of ‘effective’ boat launching lanes (number) | -1.7 |
| Demand satisfaction for ‘effective’ boat launching lanes | 250% |
| State-wide demand satisfaction for ‘effective’ boat launching lanes | 87% |

Demand summary


The assessment of recreational boating demand is centred on a statistical demand model that considers vessel registration data, population statistics, assumptions around local usage and the movement of vessels into and out of the LGA. Key parameters from this assessment for the Western Downs LGA are:

* The population is 34,197 as at the 2021 census and is projected to be 34,847 by 2041.
* As of July 2022, there is a total of 525 vessels with a home registration within the LGA, with 100% being ‘trailable’ – and therefore requiring boat launching facilities.
* The Western Downs LGA is deemed to be a Regional Centre with an assumed vessel activation rate of 8% on a ‘good boating day’.
* Vessels are primarily used within the LGA, with some leakage to Sunshine Coast, Gympie, Fraser Coast and Moreton Bay LGAs.
* There are few vessels from neighbouring LGAs that use facilities within the Western Downs LGA.
* The existing demand for boat launching facilities is 1.1 ‘effective’ boat ramp lanes and is not projected to change by 2041.

Boat launching

Boat launching facilities comprise boat ramps, any queuing facilities (floating walkways, pontoons, beaches and fixed sloping walkways) and the provision of car and trailer unit (CTU) parking. The capacity of a boat launching facility is measured in ‘effective lanes’ for both waterside and landside facilities, with the total capacity of a facility being the minimum of the waterside or landside capacity. Waterside capacity is calculated from the number of boat ramp lanes multiplied by environmental reduction factors (for tide, current or waves) and queuing facility improvement factors to derive the number of ‘effective’ lanes. The landside capacity is calculated from the number of available CTU parking spaces that are available.

Western Downs LGA has three formal boat launching facilities, comprising three boat ramp lanes with a total effective boat launching capacity of 2.8 ‘effective’ lanes. These formal facilities are supported by several informal facilities within the LGA. The Condamine facility is constrained due to parking limitations while the other two facilities are constrained by waterside capacity. The capacity and forecast demand of effective boat ramp lanes in the Western Downs LGA are shown in Figure 1.



1. Existing capacity and forecast demand of ‘effective’ boat ramp lanes for the Western Downs LGA

Priority recommendations

The capacity of boat launching facilities of Western Downs LGA is adequate for the period of this Study and no recommendations for new or upgraded facilities is required.

Contents

[Definitions 8](#_Toc132712117)

[1 Introduction 11](#_Toc132712118)

[2 Western Downs LGA Overview 12](#_Toc132712119)

[2.1 Key influences on recreational boating 12](#_Toc132712120)

[2.2 Existing recreational boating infrastructure 12](#_Toc132712121)

[3 Capacity Assessment 14](#_Toc132712122)

[3.1 Boat ramps 14](#_Toc132712123)

[4 Demand Assessment 20](#_Toc132712124)

[4.1 Activation rate 20](#_Toc132712125)

[4.2 Digital user survey 21](#_Toc132712126)

[4.3 Active fleet size 22](#_Toc132712127)

[4.4 Boat ramp lane demand 23](#_Toc132712128)

[4.5 Non-statistical demand 23](#_Toc132712129)

[5 Shortfall Assessment 25](#_Toc132712130)

[5.1 Shortfall assessment – boat ramps 25](#_Toc132712131)

[6 Stakeholder Feedback 26](#_Toc132712132)

[6.1 Managing authority feedback 26](#_Toc132712133)

[6.2 Stakeholder feedback 26](#_Toc132712134)

[7 Development Recommendations 28](#_Toc132712135)

[7.1 Previous recommendations 28](#_Toc132712136)

[7.2 Priority recommendations 29](#_Toc132712137)

[8 References 30](#_Toc132712138)

[Annex A Demand Study A-1](#_Toc132712139)

[Annex B Boat launching facility capacity B-1](#_Toc132712140)

[Annex C Facility Use C-1](#_Toc132712141)

Tables

[Table 2.1 Recreational boating facilities by facility owner in Western Downs LGA 12](#_Toc132712142)

[Table 3.1 Queuing facility efficiency modifiers 17](#_Toc132712143)

[Table 4.1 LGA of origin for active fleet in Western Downs LGA 21](#_Toc132712144)

[Table 4.2 Popularity of boat launching facilities. 22](#_Toc132712145)

[Table 4.3 Active fleet vessel size 22](#_Toc132712146)

[Table 4.4 Boat ramp lane demand 23](#_Toc132712147)

[Table 5.1 Shortfall of boat launching facilities 25](#_Toc132712148)

[Table 6.1 Stakeholder identified opportunities 26](#_Toc132712149)

[Table 7.1 Assessment of unimplemented 2017 recommendations 28](#_Toc132712150)

[Table B.1. Capacity of existing boat launching facilities B-1](#_Toc132712151)

[Table C.1. Boat launching facility usage statistics C-1](#_Toc132712152)

Figures

[Figure 2.1 Public boat launching facilities within the Western Downs LGA. 13](#_Toc132712153)

[Figure 3.1 Summary of limiting capacity constraint 19](#_Toc132712154)

Definitions

| Term | Definition |
| --- | --- |
| All‑tide (for boat ramps) | Access from a boat ramp to the open sea with an approach depth of 0.5m below LAT or deeper and a depth at boat ramp toe of 0.5m below LAT or deeper. |
| All-tide (for landings) | Access from a gangway‑access pontoon or jetty to the open sea with an approach depth of 1.5m below LAT or deeper and a depth on at least one face of the pontoon of 1.5m below LAT or deeper. |
| BIP | Boating Infrastructure Program – a sub‑program within MSQ's Maritime Assets and Infrastructure Program |
| Boat ramp | A foreshore concrete ramp with a slope designed for vehicular launching and retrieving of recreational boats. |
| Breakwater | A structure constructed over the seabed and/or the foreshore, usually rising to a height above high tide, designed to provide protection to landward areas by limiting penetration of wave action or currents. |
| CTU | Car-trailer unit space – a parking space for a typical car with a boat trailer attached. |
| Demand | Demand is the requirement of the boat‑owning population for facilities to launch/retrieve trailer boats and/or to berth suitable boats at a given year to service their average (non‑peak period) needs. In most locations demand is based on vessel registrations and is expressed in terms of boat ramp lanes or in number of 12m berths at landings. |
| Effective capacity | For a boat ramp, effective capacity (effective lanes) means the number of boat ramp lanes after adjusting for anticipated unavailability due to unacceptable wave action (>0.2m wave height) or water depth, usage constraints such as the lack of adequate parking, and improvements to efficiency or launch/retrieval throughput such as floating walkways or pontoons. |
| FHA | Fish Habitat Area, declared under the Fisheries Act, 1994 |
| FIFO | Fly‑in fly‑out, where skilled workers travel from their city or central location home communities to a remote site to perform their duties often in blocks of time that provide regular, non-weekend, days off. |
| Fixed sloping walkway | A fixed sloping structure installed at the side of a boat ramp to assist launching/retrieval of trailer boats, and dry embarkation/disembarkation from trailer boats. It is sloped to allow use at varying tide heights – sometimes with sections of different slope. |
| Floating walkway | Multiple connected/hinged flotation modules configured to assist launching/retrieval of trailer boats, and dry embarkation/disembarkation from trailer boats at most if not all stages of the tide. Floating walkways are connected to a concrete shore abutment allowing pedestrian and assisted wheelchair access. |
| Gangway access pontoon | A platform/module that always floats, where a boat can be secured alongside on one or more faces. Pontoons are usually separated from a boat ramp and have a hinged articulated gangway for access to the shore via an abutment. |
| GBR | Great Barrier Reef |
| GCWA | Gold Coast Waterways Authority |
| Landing | A landing is a jetty or gangway‑access pontoon that facilitates berthing of vessels and transfer of passengers and stores. They are most often associated with non-trailable vessels |
| Landside | Refers to areas above high-water mark, often used to denote the location of and type of infrastructure. |
| LAT | Lowest Astronomical Tide, used as Chart Datum on navigational charts. |
| LGA | Local Government Area |
| Managing authority | Councils, port authorities, water storage managers as listed in schedule 1 of the Transport Infrastructure (Public Marine Facilities) Regulation 2011 |
| MCU | Material change of use under the planning scheme |
| MNES | Matter of national environmental significance under the Environment Protection and Biodiversity Conservation Act 1999 |
| MSQ | Maritime Safety Queensland |
| NC Act | Nature Conservation Act 1992 |
| Near all‑tide | Access from a boat ramp to the open sea with a minimum approach depth of 0.5m below LAT and minimum depth at the boat ramp of 0.5m below LAT for 80 percent or more of the tidal range (time measured over a year). |
| Parking - Formalised | A sealed, line-marked parking area for car-trailer units, providing adequately sized parking spaces, roadways and turning circles. |
| Parking – Semi-formalised | An all-weather non-sealed parking area, with markers to delineate adequately sized car-trailer unit parking bays and turning circles. Markers can be concrete blocks, pavement markers (e.g., retro-reflective raised markers) or other permanent instalment to show parking bays. |
| Parking – Informal overflow | A naturally surfaced area available for use as overflow parking on the design boating day, signed as such. To have mixed-use purpose (e.g., parkland) when not being utilised as overflow parking. |
| Part‑tide | Boat ramps that do not meet near all-tide or near all-tide requirements. |
| PV | Passenger vehicle (i.e., car – as opposed to car-trailer unit). |
| Port Authority | An organisation that is responsible for the management of one or more ports on the Queensland coast. |
| Population Centre | Official named urban settlements (populated places) that have been sourced from the Queensland Place Names Database. |
| Registration activation rate | The percentage of registered vessels liable to be in use on any given good weather weekend day |
| Shortfall | The number of effective boat ramp lanes or landings required to meet demand for a given timeframe. Negative shortfall signifies an oversupply for the time period nominated. |
| SPL | Strategic Port Land |
| Study | The Recreational Boating Facility Demand Forecasting Study 2022, including this document. |
| TMR | Department of Transport and Main Roads |
| Water Storage Authority | Includes SEQwater, SunWater |
| Waterside | Refers to areas below high-water mark, often used to denote the location of and type of infrastructure, including dredged channels and breakwaters. |
| WHA | World Heritage Area |
| # | Number |

# Introduction

BMT has been appointed to undertake the Recreational Boating Facilities Demand Forecasting Study 2022 (‘the Study’) by Maritime Safety Queensland (MSQ), a branch of the Queensland Department of Transport and Main Roads (TMR), on behalf of all public recreational boating facility managers and owners across Queensland. The Study supersedes the 2017 study of the same name and is intended to report on recreational boating facility demand, capacity, and shortfall over a 20-year period at a Local Government Area (LGA) scale across Queensland.

The Study has been developed using information from the 2021 Australian Census (ABS, 2021), recreational boat vessel registrations, consultation with facility owners, managers, and stakeholders, the 2022 Queensland Government Get-Involved recreational boating facilities survey (MSQ, 2022), and previous versions of this Study (2011, 2017). The Study is intended for use by deliverers, owners, managers, and key stakeholders of public recreational boating facilities across Queensland, namely state government agencies including MSQ and the Gold Coast Waterways Authority (GCWA), local governments, port authorities and water authorities. The Study is non-regulatory in nature and is intended to be used as part of a broader suite of information to identify priority investment in recreational boating infrastructure at a local and state level.

The Study establishes demand primarily on statistics derived from registration and population data. However, non-statistical forms of demand may also be reflected in Study recommendations. The Study evaluates existing and forecast demand over a 20-year period and makes recommendations on how this demand might be met over that period. Recommendations may include improvements to both landside and waterside capacity depending on the facility.

Recommendations are assigned a priority ranking, from 1 to 4, indicating if they are required immediately or in the next 5, 10 or 15 years respectively. To end 2022, 14% of recommendations from the 2017 study have been completed, comprising 11% of landside recommendations and 18% of waterside recommendations and reflecting 22% of priority 1 2017 recommendations. A much greater percentage of the earlier 2011 study recommendations have now been implemented. Given the low uptake on existing/outstanding recommendations, this Study reviews previous recommendations and carries forward, modifies, or removes as appropriate. The Study has also been tasked with reviewing specific wave exposed beach launching facilities across the state to determine their contribution to meeting boating facilities demand and make recommendations about their future.

The Study includes a report for every LGA in Queensland and a state-wide summary report. Each LGA report summarises demand pressures from vessel registration data, population statistics, assumptions around local usage and the movement of vessels into and out of the LGA, and existing capacity and recommends opportunities to satisfy shortfall. The state-wide report will support the LGA reports and provide context at a state level for demand pressures, current capacity, equity of access to facilities and state-wide priority for major boating facilities.

The Study is intended to report on publicly accessible recreational boating facilities for registered vessels. This includes boat ramps, floating walkways, pontoons, fixed sloping walkways and supporting car and trailer parking at each facility. The Study does not include recommendations for facilities that are used primarily for commercial purposes, private facilities, non-motorised recreation such as launching canoes and stand-up paddle boards, and fishing platforms.

# Western Downs LGA Overview

## Key influences on recreational boating

Within the Western Downs LGA, the principal attributes and influences that affect demand on recreational boating infrastructure include:

* its designation as a Regional Centre, with a small local recreational boating fleet
* a stagnant projected population
* limited inflow of vessels from other LGAs
* drought and rain cycles which impact the usability of the water bodies in the LGA.

## Existing recreational boating infrastructure

The recreational boating facilities within the Western Downs LGA are summarised in Table 2.1. These facilities are owned and managed by TMR and include facilities that provide access to freshwater.

Recreational boating facilities by facility owner in Western Downs LGA

| Owner | Other boat ramps | | Landings | |
| --- | --- | --- | --- | --- |
| Facilities | Lanes | Pontoons | Jetties |
| TMR | 3 | 3 | 1 |  |

Each of the boat launching facilities within the LGA is shown in Figure 2.1.



Public boat launching facilities within the Western Downs LGA.

"I:\A12068\_TMR\_Rec.Boating.Demand.Forecast.Study\QGIS\ReportFigures\WesternDowns\A12068\_002\_GIS\_WesternDownsBoatLaunchingFacilities.jpg"

# Capacity Assessment

## Boat ramps

* + 1. Introduction

Boat ramps are facilities that are used for launching and retrieving trailable vessels, typically up to 8m in length (with some exceptions), to and from the water. Boat ramps consist of one or more lanes and are often supported by landside and waterside infrastructure to improve facility efficiency. In some instances, the usability of a facility is adversely affected by environmental constraints such as tide levels, currents, or wave exposure, reducing the overall availability of the facility. Together, consideration of the number of boat ramp lanes, the supporting infrastructure, and environmental constraints results in the facility having a capacity described in terms of ‘effective lanes’ that may or may not be equal to the number of actual boat ramp lanes. The landside and waterside capacity of each facility needs to be balanced. Each facility will have a calculated ‘effective’ capacity for both the landside and waterside elements, with the limiting element dictating the facility's overall effective capacity. Assessment and recommendations promote balancing the two elements by improving the limiting element for increased facility effectiveness or increasing the 'effective capacity' in a balanced way through changes to both elements.

* + 1. Boat ramp capacity

The waterside capacity is informed by the number of boat ramp lanes and the number and type of queuing facilities, such as pontoons, floating walkways, queuing beaches and fixed sloping walkways. It may also be limited by the available water depth in the adjacent waterbody and exposure to environmental or other physical factors.

Landside capacity is governed by the availability of nearby car-trailer unit (CTU) spaces for parking, the provision of rigging and de-rigging facilities, and provision of single car parking spaces (single cars may otherwise be obliged to park in CTU spaces).

While it is expected that facilities will have their own characteristics influencing efficient use, this Study applies an approach that is consistent across the entire state and consistent with previous editions of the Study. Accordingly, the effective waterside capacity of a boat launching facility is determined as being:

* the ability to support 40 vessels being launched and retrieved per day per lane (see section 3.1.3)
* influenced by exposure to wave, tide, and current conditions (see section 3.1.4)
* supported by queuing facilities that assist in the efficient use of the boat ramp (see section 3.1.4).

Calculation of landside capacity is in line with the TMR guideline (TMR, 2020), which requires less provision of CTU parking per lane than the Australian standard (AS3962 Table 7.1), which advises:

* 10 CTUs for a single lane boat ramp accessed by an unsealed road, or 15 CTUs accessed by a sealed road
* 45 CTUs for a two-lane boat ramp
* 70 CTUs for a three-lane boat ramp
* 90 CTUs for a four-lane boat ramp.

A notable difference from the 2017 study is the recognition and inclusion of areas close to existing boating facilities that are unsealed and/or not line marked where parking of cars with trailers occurs and is not discouraged. These areas of informal parking have been identified on aerial imagery and through discussions with managing authorities. Each informal area has been assumed to be available for CTU parking only 50% of the time to account for conflicts with other uses (for example, markets), inefficient parking practices, or poor ground conditions. The rate of parking has been calculated as:

* for linear areas where nose-to-tail parking is expected – 1 CTU per 13m
* for linear areas with enough space to allow side-by-side parking – 1 CTU per 3m, provided there is a minimum distance of 15m from the road or manoeuvring area
* for large areas – 1 CTU per 100m2.
  + 1. Boat ramp capacity basis

The number of vessels per day each boat ramp lane can support is based on the Australian Standard for the Design of Marinas (AS3962-2001) and previous versions of this report (GHD, 2011 and 2017).

Research on boat ramp lane efficiency described in the previous report (GHD, 2017) identified that 40 vessels per lane per day was a reasonable compromise between 50 vessels per lane per day (representing congested conditions) and 30 vessels per lane per day (representing unhampered conditions). For context, the 40 vessels per lane per day rate represents a vessel launch or retrieval every 9 minutes per lane within an average normally used period of 12 hours per day.

During this Study, BMT has sought to validate the assumptions presented above, and those relating to capacity modification, by undertaking a literature review, conducting site visits that included observations of launching and retrieving manoeuvres, and reviewing video recordings of boats launching and retrieving at popular boating facilities. The literature review included a boat ramp efficiency investigation undertaken by BMT on the Mornington Peninsula, Victoria (BMT, 2015) and a review of standards from other Australian states and countries that undertake similar studies. The onsite and video analysis provided the opportunity to observe recreational boat operators using facilities included in the Study but did not include observation of total throughput during high demand periods. This assessment was undertaken during site visits across Queensland, and a full day of video recording at Manly Boat Harbour (north ramp) in Brisbane.

The New South Wales and Victoria governments are currently in a planning phase for boating infrastructure and there are presently no publicly accessible documents identifying how those jurisdictions calculate boat ramp lane capacity. The Western Australia government has commissioned studies of the Perth region and the southwest region (Western Australia Department of Transport, 2019 and 2021) that indicate a base rate of 50 vessels per lane per day, with no modifiers applied. Internationally, studies from Florida in the USA (Bell, 2022 and Swett et. al, 2012) assumed that total vessel launch plus retrieval time is between 20 to 40 minutes (18 to 36 vessels per day), although no evidence is provided to support this assumption.

The Mornington Peninsula report (BMT, 2015) collected boat launch and retrieval data for 6 boat ramp facilities on the Mornington Peninsula across 9 days, including the peak Australia Day holiday. Total throughput was assessed for each facility on days where there was constant pressure for launching and retrieving boats with results between 30 and 70 vessels per lane per day for the various facilities. When adjusted for queuing modifications, a baseline rate of between 20 and 50 vessels per lane per day was identified. Of the facilities, the higher rates were achieved where sufficient parking was provided and both waterside and landside queuing facilities existed.

Observations of recreational boat users launching and retrieving their vessels undertaken through the site visits and the analysis of video footage showed that:

* Most observed launches were of ‘multi-person’ boats, which made launching and retrieving boats more efficient.
* Almost all users were able to launch and/or retrieve their boat within the 9-minute target time, when adjusted for queuing facility efficiency.
* There was a preference to launch adjacent to a floating walkway, where one was available. At facilities where a queuing facility is not immediately adjacent to the lane it is expected that average launch times may slightly increase during busy periods.

While the observations that were made generally aligned with expectations, a more in-depth review of capacity assumptions was outside of the scope of the Study. For future studies there would be value in undertaking a more thorough, data-driven investigation of the assumptions about boat ramp lane capacity, both at its base level and modified by queuing facilities. Overall, the preliminary investigations undertaken as part of the Study suggest that the base rate of 40 vessels per lane per day adopted in previous studies is appropriate.

* + 1. Boat ramp efficiency modifications

The waterside capacity of boat ramp lanes can be reduced by environmental factors that include:

* Water levels: Mainly relating to tidal areas this factor considers the reduction in the amount of time the boat ramp is available to launch and retrieve vessels over the full tidal cycle, thus reducing the overall capacity of the facility. For all-tide access, the boat ramp and connecting channel to the open sea is available during all tidal conditions and therefore available 100% of the time. For near all-tide access the boat ramp and the connecting channel to the open sea is assumed to be available, on average, for 80% of the tidal cycle. For part-tide access the boat ramp and its access channel is available less than 80% of the time. A modification factor of 0.8 is applied for near all-tide facilities and 0.5 for part-tide facilities.
* Wave and current conditions: In areas where vessel launching and retrieval may be intermittently impacted by waves (most commonly on beach ramps, but not exclusively) or strong currents (such as in rivers), a modification factor of 0.5 is applied.

Conversely, effective boat ramp capacity can be improved through the use of well-designed queuing facilities. Queuing facilities aim to improve amenity and efficient use of the boat ramp by accelerating one or more of the following phases of boat launching, with the opposite steps required for retrieval:

1. manoeuvring for launching, including for CTU entering the queuing area for the boat ramp and reversing into position for launch
2. launching and securing the launched vessel
3. moving the launch vehicle from the boat ramp to the parking area
4. removing the vessel from the waterside queuing facility.

A range of waterside queuing facilities is in use in Queensland boating infrastructure, which modify different phases of the total launching process. These include:

* Floating walkways and fixed sloping walkways: Positioned to abut a boat ramp lane, these structures aim to:
  + improve amenity – such as to assist embarking/disembarking passengers, provide a refuge from in-water contact with crocodiles and so on
  + make securing the vessel and removing the vehicle from the boat ramp more rapid, while freeing the boat ramp for subsequent users.
* Pontoons: Also used by deep-draught vessels, these structures improve the ability to secure the vessel and clear the boat ramp, but there is usually some time lost returning to recover the launch vehicle compared with the above options as they are generally positioned slightly further away from the ramp.
* Queuing beaches: These also provide a place to secure the vessel close to the boat ramp, although these are generally not as fast to use as pontoons.

As observed throughout the Study site visits, each of these queuing facility types can support a limited number of boat ramp lanes depending on the available space on the queuing facility. The 2017 edition of this Study applied a blanket uplift for all boat ramp lanes where a queuing facility was provided. However, the number of lanes each type of queuing facility can realistically support varies. Accordingly, this Study has provided limitations to the number of boat ramp lanes that can benefit from each queuing facility, based on the number of “working faces” (or area for a queuing beach) provided, where the “working face” is a face that allows temporary securing of vessels during launching or retrieval. The adopted improvement factors and supported lanes are summarised in Table 3.1.

Queuing facility efficiency modifiers

| Queuing facility | Modification factor | Supported lanes |
| --- | --- | --- |
| Floating walkway (lanes adjacent to walkway) | 1.7 | 1 Lane/face |
| Floating walkway (lanes not adjacent to walkway) | 1.3 | 1 Lane/face |
| Fixed sloping walkway | 1.2 | 1 Lane/face |
| Pontoon | 1.2 | 2 Lanes/face |
| Queuing beach | 1.15 | Site-based |

In other states in Australia, reversing queuing bays are more commonly used than in Queensland. These are CTU waiting bays at the head of the boat ramp that are aligned with each boat ramp lane to allow the user to reverse directly down the boat ramp once it is clear. CTU waiting bays reduce the time of the first phase of boat launching by allowing waiting CTU’s to be ready to reverse as soon as the lane becomes clear. The BMT (2015) study on the Mornington Peninsula included facilities with and without these bays. Boat ramps that included reversing queuing bays achieved 50% greater throughput. Facilities that have implemented this approach in Queensland include North Street Southport, Urangan Boat Harbour, Townsville Recreational Boating Park, and the (under construction late 2022) boat ramp at Yorkeys Knob.

* + 1. Accessibility from boat launching facilities

Recreational boat users will typically select the boat launching facility most appropriate or convenient to the activity they are seeking to undertake, the anticipated weather/wave conditions, and their destination. Each of facility within an LGA will provide a varying degree of access to different destinations and for different activities. During the Study, consultation with stakeholders highlighted the following general types of destinations and activities:

* open water/offshore: typically accessed for visiting offshore islands or remote beaches, snorkelling or diving locations, deep sea fishing and general recreation
* creeks and estuaries: typically accessed for fishing, crabbing, wildlife observation, skiing and general recreation
* freshwater: typically accessed for skiing, fishing, wildlife observation and general recreation.

These destinations are typically serviced by different types of recreational vessels. Inshore locations including creeks, estuaries and other freshwater locations are typically patronised by vessels less than 4.5m, except for ski boats, which can be much larger than this. Offshore locations typically require larger boats for access as these vessels are more capable of managing a wide range of wave conditions and can carry sufficient fuel to access distant destinations. Smaller vessels may be able to access close destinations on good weather days, and larger vessels may choose to access inshore destinations, particularly on poor weather days.


Consequently, the following aspects are used to classify how well a facility provides open water access:

* Open-water access: There are no restrictions between the facility and open water.
* Depth-limited access: There are depth restrictions between the facility and open water that limit navigable access to part of the tidal range. This differs from tidal constraints at the actual facility, which might be usable at all tides, but offshore access is limited by a downstream bar or delta.
* Distance-limited access: The distance from the facility to the open water is unrealistic for typical boat users. This distance is assumed to be about 4.5km between the facility and open water to rate as 'distance limited', with travel times increased further where portions of the access channel are regulated by speed limits.
* Infrastructure-limited access: There are man-made obstacles between the facility and open water, such as above-ground pipeline crossings, low bridges or weirs that impede navigable access to open water.
* Beach ramps: These provide open-water access but are typically constrained by environmental conditions such as wave exposure and tide levels. The capacity of these facilities has been individually assessed based on consultation and other data sources and is described in more detail in section 4.
* Freshwater: There is no access to open water.

Certain facilities, particularly those in freshwater, may be constrained by periods of drought, or debris deposition after rainfall events that limit access to destinations, and therefore whether a facility will provide useful boat launching capacity. While it is noted that drought and rainfall may affect the overall capacity of boat launching within an LGA and given that the timing of such events is not readily predictable, their impact on capacity has not been evaluated.

* + 1. Existing boat launching capacity

Within the Western Downs LGA there are three boat launching facilities with a total effective capacity of 2.75 lanes. The effective capacity of boat launching facilities within the Western Downs LGA is shown in Annex B, with the overall capacity constraint shown in Figure 3.1.



Summary of limiting capacity constraint

* + 1. Informal boating facilities

Consultation with the Western Downs Regional Council identified several informal facilities that are used by recreational boats across the LGA but are not maintained by the council. These facilities are located at the following locations

* Lake Broadwater: This facility is used during the water-skiing season and can be constrained due to shallow water caused by water level fluctuations.
* Jandowae: Accesses a local water body that allows water-skiing for up to 3 boats at a time.
* Miles – Pump Station Road: Access to a small creek to the south of Miles.

# Demand Assessment

The Study has developed a model to calculate statistical demand for boat launching facilities and deep draught vessel landings at an LGA scale. Vessels that are less than 8m in length are considered trailable and drive demand for boat launching facilities such as boat ramps, while those over 8m are assumed to remain on water and drive demand for deep draught landings.

Statistical demand is recognised at three different levels for public marine facilities within the TMR guidelines (TMR, 2020), which are:

* off-peak demand – typical weekday usage
* average demand – demand on ‘good boating days’, taken to be demand for a facility on weekends (and, for certain regional locations, other busy periods)
* peak demand – demand for a facility at peak holiday periods or for special events.

The demand model created for this Study is intended to provide information on demand pressures on ‘good boating days’ for all facilities as per the intentions of the guidelines. The model achieves this through a ‘registration activation rate’ that estimates the proportion of registered vessels in an LGA that are assumed to be active on a ‘good boating day’, as well as the exchange of vessels between LGAs, and general tourism pressures.

## Activation rate

The fleet size for each LGA is determined statistically from vessel registration numbers and the application of a vessel activation rate, while for future time horizons vessel registration and population growth estimates are also utilised. The methodology for determining the registration activation rate has been adopted from the previous study (GHD, 2017), with activation rates taken to be between 8% and 14% for a typical weekend. The variability of the activation rate is intended to capture the regional differences in vessel types, and is driven by the availability of access to open water, accessibility of other recreational opportunities, and likelihood of users’ available time for recreation, considering factors including:

* remoteness classification for the LGA
* incidence of blue-collar employment
* average age of residents
* whether the LGA is coastal.

Further information about the derivation of this rate can be found in Annex A. For the Western Downs LGA the activation rate is assumed to be 8%, with the key factors influencing the rate including:

* its classification as a Regional Centre
* the incidence of blue-collar employment is higher than the state average.
* the average age is lower than the state average.

## Digital user survey

To gain an understanding of usage trends at existing formal recreational boating facilities across Queensland, the Study has considered the results of a digital user survey using human movement data, sourced through a third party. The data was acquired from a location data store with more than 13 trillion mobile location observations globally from 2019 to present, which were sourced from 250,000 different mobile phone applications that users ‘opted-in’ to use the location services under the application’s terms and conditions. All data received was deidentified and compliant with relevant data privacy regulations.

The analysis uses mobile devices (such as telephones) location data as a proxy for boat user traffic, however, this relationship has several limitations including, but not limited to:

* Mobile device users detected in the area of interest may not be boat users (for example, pedestrians not using vessels may walk through the detection area).
* The relationship between mobile device users and vessels may not be 1:1 (that is, there may be multiple mobile devices providing data for each vessel).
* Users of vessels may not have a mobile device, may not be using a mobile device or may not have provided permission to use their location data.

With these, and potentially other, limitations in mind, the Study compared this data against vessel launching counts provided by various facility managers and found that approximately 15-30% of vessels are captured using this digital survey method. This percentage can change from facility to facility and from day to day. Consequently, the Study has not relied on raw counts of users from this data, but instead considered the relative trends within the data, with the assumption that no groups (for example, users from a particular LGA or using a particular facility) within the data would be more or less likely to be captured by the technique.

The Study has used this data to identify the relative volume of users, the ‘home’ local government area of users and the popularity of destinations that users travel to once vessels have been launched.

* + 1. Inter-LGA demand

The human movement data has been interrogated to determine the LGA of origin for users of the Western Downs LGA’s public boating facilities to indicate the proportion of users from each LGA that are using specific facilities. Statistics from all public boating facilities within the LGA are then grouped together to determine the total proportion of resident or visiting users across the LGA. Table 4.1 shows the active fleet proportion from the top 10 LGAs contributing to demand on facilities within the Western Downs LGA. All other sources have been grouped together.

LGA of origin for active fleet in Western Downs LGA

| LGA of origin | Active fleet proportion |
| --- | --- |
| Western Downs | 51.30% |
| Brisbane | 8.00% |
| Toowoomba | 5.60% |
| Sunshine Coast | 3.90% |
| Moreton Bay | 3.20% |
| Gold Coast | 3.10% |
| Redland | 2.80% |
| Logan | 2.20% |
| Ipswich | 1.80% |
| Fraser Coast | 1.30% |
| Other LGAs | 16.70% |

* + 1. Intra-LGA demand distribution

Recreational boating users will tend to use facilities that best suit their needs, the destinations they want to access, the capability of their vessel and the weather conditions. Consequently, distribution within an LGA is unlikely to be evenly spread across all facilities, with some facilities attracting users disproportionately due to amenity, access, or destinations. The attractiveness of large well-designed facilities is likely to draw visiting boat users in preference to smaller or less desirable facilities across the LGA. The human movement statistics have been assessed to qualitatively estimate the proportion of users using each facility, both in total and with respect to both resident and visiting boat users (Table 4.2).

Popularity of boat launching facilities.

| Facility | Overall fleet | Resident fleet | Visiting fleet |
| --- | --- | --- | --- |
| Chinchilla Weir - Chinchilla Tara Road | 72.7% | 81.7% | 63.1% |
| Condamine, Caliguel Lagoon | 18.9% | 12.0% | 26.2% |
| Chinchilla Weir - Archers Crossing Road | 8.4% | 6.3% | 10.7% |

The results indicate that the Chinchilla Weir, Chinchilla Tara Road facility is the most popular amongst locals and resident recreational boat users. The visiting fleet used the Condamine facility at a higher proportion than the local fleet, although this impact is expected to be mild given the relatively low numbers of boats.

## Active fleet size

The total ‘active’ fleet on a good boating day is derived from the activation rate of the total fleet of registered vessels within the LGA and the net inflow of visiting vessels. The total number of visiting vessels from each LGA is determined from the number of vessels in the resident active fleet and the relative proportion of resident to visiting vessels outlined in Table 4.1.The fleet size is expected to change over time due to changes in population and vessel acquisition trends, with the size and proportion of the fleet across the Study period described in Table 4.3.

Active fleet vessel size

| Vessel length | 2021 | 2026 | 2031 | 2036 | 2041 |
| --- | --- | --- | --- | --- | --- |
| 0 to 4.5m | 29 | 29 | 30 | 30 | 30 |
| 4.5m to 8m | 13 | 13 | 14 | 14 | 14 |
| >8m | 0 | 0 | 0 | 0 | 0 |
| Total | 42 | 43 | 43 | 44 | 44 |

## Boat ramp lane demand

The fleet size derived in Table 4.3 represents the statistical demand for the LGA, with vessels under 8m assumed to contribute to boat ramp demand, measured in boat ramp lanes. As outlined in section 3.1.2 the adopted capacity of each effective lane is 40 vessels per day, with each vessel assumed to both launch and retrieve, for a total of 80 vessel movements per day. The total boat ramp lane demand across the Study period is shown in Table 4.4.

Boat ramp lane demand

|  | 2021 | 2026 | 2031 | 2036 | 2041 |
| --- | --- | --- | --- | --- | --- |
| Boat ramp lane demand | 1.1 | 1.1 | 1.1 | 1.1 | 1.1 |

For the Western Downs LGA the important elements that contribute to the boat ramp lane demand include:

* a small sized local fleet of trailable vessels
* limited inflows from other regions on regular days, peak days for particular events may see higher influx.

## Non-statistical demand

As well as the statistical demand outlined in the section above, facilities may face demand pressures that are related to their functional use, which reduces the capability of the facility to service the recreational boat fleet in the desired manner. Issues with specific facilities have been identified within the consultation process of the Study with appointed managers and other stakeholders. While care has been taken to identify these non-statistical demand issues throughout the Study, it is beyond the scope of the Study to individually review the functionality, safety, and amenity of each facility across Queensland. Non-statistical demand pressures may warrant upgrades to facilities even where statistical demand is satisfied by existing capacity. These pressures have been classified into the following categories:

* Amenity: Amenity describes the functional usability of the facility including the desire to provide dry entry and exit facilities, facilities that provide easy access and/or access for persons with restricted mobility.
* Safety: Safety demand may include protection from currents and waves or contact with marine creatures such as sharks, jellyfish, and crocodiles.
* In-water congestion: Where existing queuing facilities are not able to efficiently meet the needs of the facility. Such deficiency may warrant additional queuing facility capacity to optimise boat launching and retrieval.

The Study's recommendations may alleviate these non-statistical demand pressures with consideration for capability of all facilities within the LGA. The presence of a non-statistical demand pressure at a facility may not warrant upgrades where other suitable facilities are reasonably available.

# Shortfall Assessment

## Shortfall assessment – boat ramps

The shortfall of boat ramp lanes within the Western Downs LGA is provided in Table 5.1. The demand is stable for the period of this Study, with the capacity provided by formal boating facilities sufficient for this demand. Informal facilities add to the capacity provided by the formal facilities and increase the demand satisfaction.

Shortfall of boat launching facilities

| Metric | 2021 | 2026 | 2031 | 2036 | 2041 |
| --- | --- | --- | --- | --- | --- |
| Demand | 1.1 | 1.1 | 1.1 | 1.1 | 1.1 |
| Capacity | 2.8 | 2.8 | 2.8 | 2.8 | 2.8 |
| **Shortfall** | **-1.7** | **-1.7** | **-1.7** | **-1.7** | **-1.7** |

# Stakeholder Feedback



The Study has undertaken extensive consultation throughout its execution to achieve a comprehensive understanding of issues relating to the use of recreational boating facilities across the State. This consultation was conducted with managing authorities that own and/or and manage recreational boating facilities, as well as with facility stakeholders including recreational groups, volunteer marine rescue and coastguard organisations and the general public. Stakeholder engagement was also supplemented with site visits to facilities where key issues had been identified.

## Managing authority feedback

For the Western Downs LGA, the Study team met with the Western Downs Regional Council and Maritime Safety Queensland to discuss recreational boating facilities within the region. This consultation process discussed existing facilities and potential future improvements. The Study has considered the practical implementation of each of these opportunities with respect to the required infrastructure, difficulty of implementation and magnitude of benefit, as summarised in Table 6.1.

Stakeholder identified opportunities

| Location | Stakeholder opportunity | Review comments |
| --- | --- | --- |
| Chinchilla Weir - Chinchilla Tara Road | Duplication of this ramp is the most desirable location for future upgrades. Not needed immediately. | Agreed. This site is the most appropriate for future expansion given its proximity to Chinchilla. At this point there is no statistical basis to commit to this upgrade. |
| Chinchilla Weir - Archers Crossing Road | No requirement to upgrade | Agreed. |
| Condamine, Caliguel Lagoon | Limited by on-water capacity, no desire to upgrade. | Agreed. |
| Lake Broadwater | Informal access only, no desire to upgrade due to shallow water levels and wetting/drying cycles. | Agreed. |

## Stakeholder feedback

Broader stakeholder feedback has been conducted within the Study by undertaking virtual or face-to-face meetings with recreational boating groups and marine rescue organisations, as well as through the Recreational Boating Facility Survey (MSQ, 2022) undertaken by Maritime Safety Queensland that included survey responses of nearly 3,000 users and open submissions. For Western Downs LGA a total of 4 submissions was received, with 67% of respondents using trailable power boats and 75% of respondents using recreational boating facilities at least once a month. For Western Downs LGA the following statistics or themes were extracted from the survey and associated comments:

* 25% of respondents typically travel less than 1hr to their preferred boat ramp (which may not be their closest facility).
* 50% of respondents indicated that floating walkways are their preferred type of queuing facility.
* 75% of respondents indicated that they would be unwilling to walk further than 200m from designated CTU parking to a boat ramp.
* The most common requests for new boat ramps were at:
  + Moraby Park, opposite Swagsman Motor Inn, Miles
  + Condamine River, Condamine Township
  + Dogwood Creek
  + Warra Weir.
* The following themes were identified with respect to existing facilities:
  + Upgrading to larger facilities with pontoons (Miles Bridge)
  + Providing lighting and wash-downs.
* Where the closest available boat launching facility was not preferred, respondents indicated that the following key aspects influenced their choice:
  + Limited options to choose local boat ramps.
* Respondents were given an opportunity to provide additional feedback, with the following theme identified:
  + a desire for more boat ramps around the region to reduce the travel time to access a facility.

# Development Recommendations

## Previous recommendations

The 2017 GHD assessment recommended opportunities for increasing the capacity of recreational boating facilities across the State. However, the implementation of these recommendations has been poor, with only 10% of the total recommendations delivered in part or full in the 5 years since the delivery of the report. Of the priority 1 recommendations (for immediate delivery) and priority 2 recommendations (for implementation within 5 years) only 18% and 6% respectively have been delivered. State-wide only 5% of landside recommendations were delivered, while 16% of waterside recommendations were delivered.

Within the Western Downs LGA no recommendations have been implemented since the delivery of the 2017 GHD study. The poor rate of implementation of these recommendations is likely the result of budgetary constraints applied due to the Covid-19 pandemic. As such, many of the recommendations proposed in the 2017 GHD study remain viable. This current Study has reviewed the unimplemented 2017 recommendations (Table 7.1) for Western Downs LGA in conjunction with stakeholders during the consultation process to identify previous recommendations that are:

* Still viable: The recommendation in its original form remains suitable for solving demand pressures.
* Still viable with modifications: The recommendation could remain viable with modifications identified throughout the consultation process.
* No longer viable: The recommendations are no longer suitable to be carried through as recommendations in this Study.

Recommendations from the 2017 study that are considered viable or viable with modifications may be carried forward into the recommendations of this Study with a suitable update to their priority status if required.

Assessment of unimplemented 2017 recommendations

| Location | Description | Assessment | Review comment |
| --- | --- | --- | --- |
| Priority 1 | | | |
| Nil |  |  |  |
| Priority 2 | | | |
| Nil |  |  |  |
| Priority 3 | | | |
| Nil |  |  |  |
| Priority 4 | | | |
| Condamine, Caliguel Lagoon | Expand ramp to 2-lanes | No longer viable | Given the significant restrictions to on-water use at this site, this recommendation should not be carried forward. |

## Priority recommendations

A review of the recreational boating needs of the Western Downs LGA indicates that there is currently no statistical basis to justify the further recommendations for upgrading existing facilities or construction of any new recreational boating facilities. The current fleet of vessels registered in the Western Downs LGA are catered for by the existing facilities and via trips to the east coast regions such as the Sunshine Coast, Gympie, Fraser Coast and Moreton Bay.

# References

Australian Bureau of Statistics (ABS), 2021, *2021 Census,* <https://www.abs.gov.au/census>

Bell, Frederick W. 2022, *Estimation of the present and projected demand and supply of boat ramps for Florida's coastal regions and counties*, Florida State University, Department of Economics.

BMT, 2015, *MPSC Managed Boating Facilities Demand and Capacity Study: Boat Ramp Modelling*

Department of Transport and Main Roads (TMR), 2020, Marine facilities and infrastructure plan.

GHD, 2011, *Recreational Boating Facilities Demand Forecasting Study*

GHD, 2017, *Queensland Recreational Boating Facilities Demand Forecasting Study 2017.*

Maritime Safety Queensland (MSQ), 2022, *Recreational Boating Facilities,* <https://www.getinvolved.qld.gov.au/gi/consultation/8850/view.html>

Queensland Government Department of Resources (DoR), 2022, *Cities and towns [OGC WMS Service]*, Accessed 5/10/2022, available online at spatial.information.qld.gov.au/arcgis/home/item.html?id=103c7c9ccca449fab79d27cde06868ab

Rose, T., R. Powell & J. Yu (2009). Identification of the Present and Future Recreational Boating Infrastructure in Redland City – A 10 Year Infrastructure Plan- Griffith University

SKM (1998) Public Boat Ramps Central Queensland Strategic Plan - Volume One - Demand Forecasting - Noosa to Yeppoon. Sinclair Knight Merz, March 1998.

Swett, R., Fik, T., Ruppert, T., Davidson, G., Guevara, C. & Betty Staugler, 2012, *Planning for the future of recreational boating access to charlotte county waterways: 2010 – 2050*, Florida Sea Grant, University of Florida.

Western Australia Department of Transport, 2019, *Perth Recreational Boating Facilities Study Review 2019*, https://www.transport.wa.gov.au/mediaFiles/marine/MAC\_P\_Perth\_RBFS\_study\_review\_2019.pdf

Western Australia Department of Transport, 2021, *South West Region Recreational Boating Facilities Study July 2021,* https://www.transport.wa.gov.au/mediaFiles/marine/MAC\_P\_SouthWest\_RBFS\_Study\_2021.pdf

###### Demand Study

"G:\Admin\A12068.g.mpb.TMRBoatingDemand\06\_Reports\09\_Demand Study\2022\_2119 (016) Final Demand Report (March 2023).pdf"

###### Boat launching facility capacity

Capacity of existing boat launching facilities

| Facility ID | Facility name | No. lanes | Tidal access  (at ramp) | Queuing facility | Formal CTUs | Informal CTUs | Waterside capacity | Landside capacity | Effective capacity | Constraint |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **No Open Water Access** | | | | | | | | | | | |
| CH12 | Chinchilla Weir - Archers Crossing Road | 1 | Fresh water | None | 10 |  | 1 | 1 | 1 | Waterside |
| CH11 | Chinchilla Weir - Chinchilla Tara Road | 1 | Fresh water | None | 32 |  | 1 | 1.75 | 1 | Waterside |
| ML11 | Condamine, Caliguel Lagoon | 1 | Fresh water | None | 0 | 10 | 1 | 0.75 | 0.75 | Landside |
| **Sub Total** |  | **3** |  |  | **42** | **10** | **3** | **3.5** | **2.75** |  |
| **Total effective capacity** | | | | | | | | | **2.75** |  | |

###### Facility Use

Boat launching facility usage statistics

| Facility ID | Facility name | Total reports | Bundaberg | Brisbane | Fraser Coast | Moreton Bay | Sunshine Coast | Logan | Gold Coast | Gladstone | South Burnett | Toowoomba | Other LGAs |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Total |  | 713 | 366 | 57 | 40 | 28 | 23 | 22 | 20 | 16 | 13 | 9 | 119 |
| Total % |  | 100% | 51.3% | 8.0% | 5.6% | 3.9% | 3.2% | 3.1% | 2.8% | 2.2% | 1.8% | 1.3% | 16.7% |
| CH11 | Chinchilla Weir - Chinchilla Tara Road | 518 | 57.7% | 6.8% | 6.0% | 2.3% | 2.7% | 3.3% | 2.3% | 1.9% | 1.7% | 1.5% | 13.7% |
| ML11 | Condamine, Caliguel Lagoon | 135 | 32.6% | 10.4% | 3.7% | 10.4% | 3.0% | 3.0% | 5.2% | 4.4% | 2.2% | 0.0% | 25.2% |
| CH12 | Chinchilla Weir - Archers Crossing Road | 60 | 38.3% | 13.3% | 6.7% | 3.3% | 8.3% | 1.7% | 1.7% | 0.0% | 1.7% | 1.7% | 23.3% |

|  |  |  |
| --- | --- | --- |
|  |  | BMT is a leading design, engineering, science and management consultancy with a reputation for engineering excellence. We are driven by a belief that things can always be better, safer, faster and more efficient. BMT is an independent organisation held in trust for its employees. |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  | Contact us  enquiries@bmtglobal.com  www.bmt.org  Follow us  www.bmt.org/linkedin LinkedIn logo  www.bmt.org/youtube YouTube logo  www.bmt.org/twitter Twitter logo  www.bmt.org/facebook Facebook logo |  |
|  | Level 5  348 Edward Street  Brisbane  QLD 4000  Australia  +61 7 3831 6744 |  | Registered in Australia  Registered no. 010 830 421  Registered office  Level 5, 348 Edward Street,  Brisbane QLD 4000 Australia |  |  |  |  |
|  | For your local BMT office visit www.bmt.org | | |  |  |  |  |  |